***** 2025/11/22 20:01:20 *****
QE Version                                        :4.2.0.v20250714-0546
Project Path                                      :D:\e2_studio\workspace\RA4M2_CTSU
Configuration File                                :RA4M2_CTSU
IDE                                               :e2 studio with Emulator
Emulator                                          :
MCU                                               :RA4M2 R7FA4M2AD3CFL
<< METHOD 0 >>
[Button(self) 0]
TS                                                : TS02,
[Button(self) 1]
TS                                                : TS05,

<<<< Tuning Type : Normal >>>>
System Clock Frequency (MHz)                      :90.000
PCLKB Frequency (MHz)                             :45.000
CTSU Operating Frequency (MHz)                    :22.500
Operating Voltage (V)                             :3.300
TSCAP Voltage (V)                                 :1.180
---------- Phase1 ----------
<< METHOD 0 >>
[TS02]
Measurement Value                                 : 8722
Resistance Value (ohm)                            : 560
Parasitic Capacitance (pF)                        : 27.265734
Sensor Drive Pulse Frequency (MHz)                : 0.9375

[TS05]
Measurement Value                                 : 9944
Resistance Value (ohm)                            : 560
Parasitic Capacitance (pF)                        : 31.388319
Sensor Drive Pulse Frequency (MHz)                : 0.9375


---------- Phase2 ----------
<< METHOD 0 >>
[TS02]
Sensor Drive Pulse Frequency (MHz)                : 0.9375
CTSUSNUM                                          : 1
CTSUSSDIV                                         : 4
CTSUSDPA                                          : 11
CTSUSO                                            : 110

[TS05]
Sensor Drive Pulse Frequency (MHz)                : 0.9375
CTSUSNUM                                          : 1
CTSUSSDIV                                         : 4
CTSUSDPA                                          : 11
CTSUSO                                            : 141


---------- Phase3 ----------
<< METHOD 0 >>
[Button(self) 0]
  << TS02 >>
  Measurement Value (Off)                         : 16089
  Measurement Value (On)                          : 65535
  Threshold                                       : 29667
  Hysteresis                                      : 1483

[Button(self) 1]
  << TS05 >>
  Measurement Value (Off)                         : 16900
  Measurement Value (On)                          : 65535
  Threshold                                       : 29181
  Hysteresis                                      : 1459

