FSP Configuration
  Board "Custom User Board (Any Device)"
  R7FA4M2AD3CFL
    part_number: R7FA4M2AD3CFL
    rom_size_bytes: 524288
    ram_size_bytes: 131072
    data_flash_size_bytes: 8192
    package_style: LQFP
    package_pins: 48
    
  RA4M2
    series: 4
    
  RA4M2 Family
    Enable inline BSP IRQ functions: Enabled
    Security: Exceptions: Exception Response: Non-Maskable Interrupt
    Security: Exceptions: BusFault, HardFault, and NMI Target: Secure State
    Security: System Reset Request Accessibility: Secure State
    Security: Exceptions: Prioritize Secure Exceptions: Disabled
    Security: System Reset Status Accessibility: Both Secure and Non-Secure State
    Security: Battery Backup Accessibility: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM ECC: Both Secure and Non-Secure State
    Security: SRAM Accessibility: Standby RAM: Regions 7-0 are all Secure.
    Security: BUS Accessibility: Bus Security Attribution Register A: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register B: Both Secure and Non-Secure State
    Security: Uninitialized Non-Secure Application Fallback: Enable Uninitialized Non-Secure Application Fallback
    Startup C-Cache Line Size: 32 Bytes
    OFS0 register settings: Independent WDT: Start Mode: IWDT is stopped after a reset
    OFS0 register settings: Independent WDT: Timeout Period: 2048 cycles
    OFS0 register settings: Independent WDT: Dedicated Clock Frequency Divisor: 128
    OFS0 register settings: Independent WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: Independent WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: Independent WDT: Reset Interrupt Request Select: Reset is enabled
    OFS0 register settings: Independent WDT: Stop Control: Stop counting when in Sleep, Snooze mode, or Software Standby
    OFS0 register settings: WDT: Start Mode Select: Stop WDT after a reset (register-start mode)
    OFS0 register settings: WDT: Timeout Period: 16384 cycles
    OFS0 register settings: WDT: Clock Frequency Division Ratio: 128
    OFS0 register settings: WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: WDT: Reset Interrupt Request: Reset
    OFS0 register settings: WDT: Stop Control: Stop counting when entering Sleep mode
    OFS1_SEL register settings: Voltage Detection 0 Level Security Attribution: VDSEL setting loads from OFS1_SEC
    OFS1_SEL register settings: Voltage Detection 0 Circuit Start Security Attribution: LVDAS setting loads from OFS1_SEC
    OFS1 register settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS1 register settings: Voltage Detection 0 Level: 2.80 V
    OFS1 register settings: HOCO Oscillation Enable: HOCO oscillation is disabled after reset
    Block Protection Settings (BPS): BPS0: 
    Permanent Block Protection Settings (PBPS): PBPS0: 
    Clocks: HOCO FLL Function: Disabled
    Main Oscillator Wait Time: 8163 cycles
    
  RA4M2 event data
  RA Common
    Main stack size (bytes): 0x400
    Heap size (bytes): 0x4000
    MCU Vcc (mV): 3300
    Parameter checking: Disabled
    Assert Failures: Return FSP_ERR_ASSERTION
    Clock Registers not Reset Values during Startup: Disabled
    Main Oscillator Populated: Populated
    PFS Protect: Enabled
    C Runtime Initialization : Enabled
    Early BSP Initialization : Disabled
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Populated: Populated
    Subclock Drive (Drive capacitance availability varies by MCU): Standard/Normal mode
    Subclock Stabilization Time (ms): 1000
    
  Clocks
    XTAL 12000000Hz
    HOCO 20MHz
    PLL Src: XTAL
    PLL Div /2
    PLL Mul x30.0
    PLL2 Src: XTAL
    PLL2 Div /1
    PLL2 Mul x20.0
    Clock Src: PLL
    CLKOUT Src: HOCO
    UCLK Src: PLL2
    ICLK Div /2
    PCLKA Div /2
    PCLKB Div /4
    PCLKC Div /4
    PCLKD Div /2
    FCLK Div /4
    CLKOUT Div /1
    UCLK Div /5
    
  Pin Configurations
    R7FA4M2AD3CFL.pincfg -> g_bsp_pin_cfg
      AVCC0 42 ANALOG0_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 43 ANALOG0_AVSS0 - - - - - - - - IO "Read only" - 
      P000 48 ADC0_AN000 - - - "Analog mode" - None "ADC0: AN000; ICU0: IRQ06" - IO - - 
      P001 47 - - - - Disabled - - "ADC0: AN001; ICU0: IRQ07" - None - - 
      P002 46 GPIO - - None "Output mode (Initial Low)" CMOS - "ADC0: AN002; ICU0: IRQ08" - IO - - 
      P013 40 GPIO - - - "Input mode" - None "ADC0: AN011; ANALOG0: VREFL" - IO - - 
      P014 39 DAC0_DA0 - - - "Analog mode" - None "ADC0: AN012; DAC0: DA0" - IO - - 
      P015 38 - - - - Disabled - - "ADC0: AN013; DAC1: DA1; ICU0: IRQ13" - None - - 
      P100 36 - - - - Disabled - - "AGT0: AGTIO0; GPT_POEG0: GTETRGA; GPT5: GTIOC5B; ICU0: IRQ02; QSPI0: QSPCLK; SCI0: RXD0; SCI0: SCL0; SCI1: SCK1" - None - - 
      P101 35 GPT5_GTIOC5A - Low None "Peripheral mode" CMOS None "AGT0: AGTEE0; GPT_POEG1: GTETRGB; GPT5: GTIOC5A; ICU0: IRQ01; QSPI0: QIO1; SCI0: SDA0; SCI0: TXD0; SCI1: CTSRTS1" - IO - - 
      P102 34 - - - - Disabled - - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT_OPS0: GTOWLO; GPT2: GTIOC2B; QSPI0: QIO0; SCI0: SCK0" - None - - 
      P103 33 GPT2_GTIOC2A - Low - "Peripheral mode" CMOS None "AGT2: AGTIO2; CAN0: CTX0; GPT_OPS0: GTOWUP; GPT2: GTIOC2A; QSPI0: QIO3; SCI0: CTSRTS0" - IO - - 
      P104 32 GPIO - Low None "Output mode (Initial Low)" CMOS - "AGT2: AGTEE2; GPT_POEG1: GTETRGB; GPT1: GTIOC1B; ICU0: IRQ01; QSPI0: QIO2" - IO - - 
      P108 25 DEBUG0_SWDIO - Low - "Peripheral mode" CMOS None "AGT3: AGTOA3; DEBUG0: SWDIO; DEBUG0: TMS; GPT_OPS0: GTOULO; GPT0: GTIOC0B; SCI9: CTSRTS9; SPI0: SSLA0" - IO - - 
      P109 26 SCI9_TXD9 - Low - "Peripheral mode" CMOS None "AGT3: AGTOB3; CGC0: CLKOUT; DEBUG0: TDO; DEBUG0: TRACESWO; GPT_OPS0: GTOVUP; GPT1: GTIOC1A; SCI9: SDA9; SCI9: TXD9; SPI0: MOSIA" - IO - - 
      P110 27 SCI9_RXD9 - Low None "Peripheral mode" CMOS None "AGT3: AGTEE3; DEBUG0: TDI; GPT_OPS0: GTOVLO; GPT1: GTIOC1B; ICU0: IRQ03; SCI2: CTSRTS2; SCI9: RXD9; SCI9: SCL9; SPI0: MISOA" - IO - - 
      P111 28 ICU0_IRQ04 - - IRQ04 "IRQ mode" - None "AGT5: AGTOA5; GPT3: GTIOC3A; ICU0: IRQ04; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCKA" - IO - - 
      P112 29 GPIO - - - "Input mode" - None "AGT5: AGTOB5; GPT3: GTIOC3B; QSPI0: QSSL; SCI1: SCK1; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA0; SSI0: SSIBCK0" - IO - - 
      P200 21 - - - - Disabled - - "ICU0: NMI" - None - - 
      P201 20 - - - - Disabled - - "SYSTEM0: MD" - None - - 
      P206 18 - - - - Disabled - - "CTSU0: TS02; GPT_OPS0: GTIU; ICU0: IRQ00; IIC1: SDA1; SCI4: RXD4; SCI4: SCL4; SCI9: CTS9; SDHI0: SD0DAT2; SPI0: SSLA1; SSI0: SSIDATA0; USB_FS0: USB_VBUSEN" - None - - 
      P207 17 - - - - Disabled - - "CTSU0: TSCAP; QSPI0: QSSL; SCI4: SDA4; SCI4: TXD4; SPI0: SSLA2" - None - - 
      P212 8 - - - - Disabled - - "AGT1: AGTEE1; CGC0: EXTAL; GPT_POEG3: GTETRGD; GPT0: GTIOC0B; ICU0: IRQ03; SCI1: RXD1; SCI1: SCL1" - None - - 
      P213 7 - - - - Disabled - - "AGT2: AGTEE2; CGC0: XTAL; GPT_POEG2: GTETRGC; GPT0: GTIOC0A; ICU0: IRQ02; SCI1: SDA1; SCI1: TXD1" - None - - 
      P300 24 DEBUG0_SWCLK - Low - "Peripheral mode" CMOS None "DEBUG0: SWCLK; DEBUG0: TCK; GPT_OPS0: GTOUUP; GPT0: GTIOC0A; SPI0: SSLA1" - IO - - 
      P301 23 - - - - Disabled - - "AGT0: AGTIO0; GPT_OPS0: GTOULO; GPT4: GTIOC4B; ICU0: IRQ06; SCI2: RXD2; SCI2: SCL2; SCI9: CTSRTS9; SPI0: SSLA2" - None - - 
      P302 22 - - - - Disabled - - "GPT_OPS0: GTOUUP; GPT4: GTIOC4A; ICU0: IRQ05; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA3" - None - - 
      P402 1 - - - - Disabled - - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC0: CACREF; CAN0: CRX0; ICU0: IRQ04; RTC0: RTCIC0; SCI4: CTS4; SSI_COMMON0: AUDIO_CLK" - None - - 
      P407 12 USB_FS0_USB_VBUS - Low - "Peripheral mode" CMOS None "ADC0: ADTRG0; AGT0: AGTIO0; CTSU0: TS03; GPT6: GTIOC6A; IIC0: SDA0; RTC0: RTCOUT; SCI4: CTSRTS4; SPI0: SSLA3; USB_FS0: USB_VBUS" - IO - - 
      P408 11 - - - - Disabled - - "AGT2: AGTOB2; CTSU0: TS04; GPT_OPS0: GTOWLO; GPT6: GTIOC6B; ICU0: IRQ07; IIC0: SCL0; SCI3: RXD3; SCI3: SCL3; SCI4: CTS4; USB_FS0: USB_ID" - None - - 
      P409 10 - - - - Disabled - - "AGT2: AGTOA2; CTSU0: TS05; GPT_OPS0: GTOWUP; ICU0: IRQ06; SCI3: SDA3; SCI3: TXD3; USB_FS0: USB_EXICEN" - None - - 
      P500 37 - - - - Disabled - - "ADC0: AN016; AGT0: AGTOA0; CAC0: CACREF; GPT_OPS0: GTIU; QSPI0: QSPCLK; USB_FS0: USB_VBUSEN" - None - - 
      RES 19 SYSTEM0_RES - - - - - - - - IO "Read only" - 
      USBDM 14 USB_FS0_USB_DM - - - - - - - - IO "Read only" - 
      USBDP 15 USB_FS0_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 2 SYSTEM0_VBATT - - - - - - - - IO "Read only" - 
      VCC 9 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 30 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCCUSB 16 USB_FS0_VCC_USB - - - - - - - - IO "Read only" - 
      VCL0 3 SYSTEM0_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 41 ANALOG0_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 45 ANALOG0_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL0 44 ANALOG0_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 6 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 31 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSSUSB 13 USB_FS0_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 4 CGC0_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 5 CGC0_XCOUT - - - - - - - - IO "Read only" - 
    
  User Events
    
  User Event Links
    
  Module "I/O Port (r_ioport)"
    Parameter Checking: Default (BSP)
    
  Module "UART (r_sci_uart)"
    Parameter Checking: Default (BSP)
    FIFO Support: Disable
    DTC Support: Disable
    Flow Control Support: Disable
    RS-485 Support: Disable
    IrDA Support: Disabled
    
  Module "ADC (r_adc)"
    Parameter Checking: Default (BSP)
    
  Module "DAC (r_dac)"
    Parameter Checking: Default (BSP)
    
  Module "Timer, General PWM (r_gpt)"
    Parameter Checking: Default (BSP)
    Pin Output Support: Enabled
    Write Protect Enable: Disabled
    
  Module "Low Power Modes (r_lpm)"
    Parameter Checking: Default (BSP)
    Standby Limit: Disabled
    
  Module "External IRQ (r_icu)"
    Parameter Checking: Default (BSP)
    
  Module "USB PCDC (r_usb_pcdc)"
    Bulk In Pipe: USB PIPE4
    Bulk Out Pipe: USB PIPE5
    Interrupt In Pipe: USB PIPE6
    
  Module "USB (r_usb_basic)"
    Parameter Checking: Default (BSP)
    PLL Frequency: Not Supported
    CPU Bus Access Wait Cycles: Not Supported
    Battery Charging: Not Supported
    Power IC Shutdown Polarity: Active High
    Dedicated Charging Port (DCP) Mode: Not Supported
    Notifications for SET_INTERFACE/SET_FEATURE/CLEAR_FEATURE: Enabled
    Double Buffering: Enabled
    Continuous Transfer Mode: Not Supported
    LDO Regulator: Not Supported
    DMA/DTC Support: DMA Disabled
    DMA/DTC Source Address: DMA Disabled
    DMA/DTC Destination Address: DMA Disabled
    USB Compliance Test mode: Disabled
    USB TPL table name: NULL
    
  Module "Flash (r_flash_hp)"
    Parameter Checking: Default (BSP)
    Code Flash Programming Enable: Enabled
    Data Flash Programming Enable: Enabled
    
  HAL
    Instance "g_ioport I/O Port (r_ioport)"
      Name: g_ioport
      1st Port ELC Trigger Source: Disabled
      2nd Port ELC Trigger Source: Disabled
      3rd Port ELC Trigger Source: Disabled
      4th Port ELC Trigger Source: Disabled
      Pin Configuration Name: g_bsp_pin_cfg
      
    Instance "g_uart9 UART (r_sci_uart)"
      General: Name: g_uart9
      General: Channel: 9
      General: Data Bits: 8bits
      General: Parity: None
      General: Stop Bits: 1bit
      Baud: Baud Rate: 115200
      Baud: Baud Rate Modulation: Disabled
      Baud: Max Error (%): 5
      Flow Control: CTS/RTS Selection: Hardware RTS
      Flow Control: Software RTS Port: Disabled
      Flow Control: Software RTS Pin: Disabled
      Extra: Clock Source: Internal Clock
      Extra: Start bit detection: Falling Edge
      Extra: Noise Filter: Disable
      Extra: Receive FIFO Trigger Level: Max
      Extra: IrDA: Enable: Disabled
      Extra: IrDA: RXD Polarity Switching: Normal
      Extra: IrDA: TXD Polarity Switching: Normal
      Extra: RS-485: DE Pin: Disable
      Extra: RS-485: DE Pin Polarity: Active High
      Extra: RS-485: DE Port Number: Disabled
      Extra: RS-485: DE Pin Number: Disabled
      Interrupts: Callback: user_uart9_callback
      Interrupts: Receive Interrupt Priority: Priority 12
      Interrupts: Transmit Data Empty Interrupt Priority: Priority 12
      Interrupts: Transmit End Interrupt Priority: Priority 12
      Interrupts: Error Interrupt Priority: Priority 12
      
    Instance "g_adc0 ADC (r_adc)"
      General: Name: g_adc0
      General: Unit: 0
      General: Resolution: 12-Bit
      General: Alignment: Right
      General: Clear after read: On
      General: Mode: Continuous Scan
      General: Double-trigger: Disabled
      Input: Channel Scan Mask (channel availability varies by MCU): Channel 0, Temperature Sensor
      Input: Group B Scan Mask (channel availability varies by MCU): 
      Interrupts: Normal/Group A Trigger: Software
      Interrupts: Group B Trigger: Disabled
      Interrupts: Group Priority (Valid only in Group Scan Mode): Group A cannot interrupt Group B
      Input: Add/Average Count: Disabled
      Input: Reference Voltage control: VREFH0/VREFH
      Input: Addition/Averaging Mask (channel availability varies by MCU and unit): 
      Input: Sample and Hold: Sample and Hold Channels (Available only on selected MCUs): 
      Input: Sample and Hold: Sample Hold States (Applies only to channels 0, 1, 2): 24
      Input: Window Compare: Window Mode: Disabled
      Input: Window Compare: Event Output: OR
      Input: Window Compare: Window A: Enable: Disabled
      Input: Window Compare: Window A: Channels to compare (channel availability varies by MCU and unit): 
      Input: Window Compare: Window A: Channel comparison mode (channel availability varies by MCU and unit): 
      Input: Window Compare: Window A: Lower Reference: 0
      Input: Window Compare: Window A: Upper Reference: 0
      Input: Window Compare: Window B: Enable: Disabled
      Input: Window Compare: Window B: Channel to compare (channel availability varies by MCU and unit): Channel 0
      Input: Window Compare: Window B: Comparison mode: Less Than or Outside Window
      Input: Window Compare: Window B: Lower Reference: 0
      Input: Window Compare: Window B: Upper Reference: 0
      Interrupts: Callback: user_adc_callback
      Interrupts: Scan End Interrupt Priority: Priority 10
      Interrupts: Scan End Group B Interrupt Priority: Disabled
      Interrupts: Window Compare A Interrupt Priority: Disabled
      Interrupts: Window Compare B Interrupt Priority: Disabled
      Extra: ADC Ring Buffer: Disabled
      
    Instance "g_dac0 DAC (r_dac)"
      Name: g_dac0
      Channel: 0
      Synchronize with ADC: Disabled
      Data Format: Right Justified
      Output Amplifier: Disabled
      Charge Pump (Requires MOCO active): Not Supported
      Internal Output: Not Supported
      ELC Trigger Source: Disabled
      Reference Voltage: Not supported
      
    Instance "g_timer0 Timer, General PWM (r_gpt)"
      General: Name: g_timer0
      General: Channel: 0
      General: Mode: Periodic
      General: Period: 1
      General: Compare Match: Compare Match A: Status: Disabled
      General: Compare Match: Compare Match A: Compare match value: 0
      General: Compare Match: Compare Match B: Status: Disabled
      General: Compare Match: Compare Match B: Compare match value: 0
      General: Period Unit: Seconds
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Disabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: False
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: False
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: 
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: 
      Input: Capture B Source: 
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: user_timer0_callback
      Interrupts: Overflow/Crest Interrupt Priority: Priority 11
      Interrupts: Capture/Compare match A Interrupt Priority: Disabled
      Interrupts: Capture/Compare match B Interrupt Priority: Disabled
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: ADC Trigger: ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger: ADC B Compare Match (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_timer2 Timer, General PWM (r_gpt)"
      General: Name: g_timer2
      General: Channel: 2
      General: Mode: Saw-wave PWM
      General: Period: 20
      General: Compare Match: Compare Match A: Status: Disabled
      General: Compare Match: Compare Match A: Compare match value: 0
      General: Compare Match: Compare Match B: Status: Disabled
      General: Compare Match: Compare Match B: Compare match value: 0
      General: Period Unit: Kilohertz
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Disabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: True
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: False
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: 
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: 
      Input: Capture B Source: 
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: NULL
      Interrupts: Overflow/Crest Interrupt Priority: Disabled
      Interrupts: Capture/Compare match A Interrupt Priority: Disabled
      Interrupts: Capture/Compare match B Interrupt Priority: Disabled
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: ADC Trigger: ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger: ADC B Compare Match (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_timer5 Timer, General PWM (r_gpt)"
      General: Name: g_timer5
      General: Channel: 5
      General: Mode: Periodic
      General: Period: 0x10000
      General: Compare Match: Compare Match A: Status: Disabled
      General: Compare Match: Compare Match A: Compare match value: 0
      General: Compare Match: Compare Match B: Status: Disabled
      General: Compare Match: Compare Match B: Compare match value: 0
      General: Period Unit: Raw Counts
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Disabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: False
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: False
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: 
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: GTIOCA Rising Edge While GTIOCB Low, GTIOCA Rising Edge While GTIOCB High
      Input: Capture B Source: GTIOCA Falling Edge While GTIOCB Low, GTIOCA Falling Edge While GTIOCB High
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: user_timer5_callback
      Interrupts: Overflow/Crest Interrupt Priority: Priority 9
      Interrupts: Capture/Compare match A Interrupt Priority: Priority 9
      Interrupts: Capture/Compare match B Interrupt Priority: Priority 9
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: ADC Trigger: ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger: ADC B Compare Match (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_lpm0 Low Power Modes (r_lpm)"
      General: Name: g_lpm0
      General: Low Power Mode: Software Standby mode
      General: Output port state in standby and deep standby: Not Supported
      General: Supply of SOSC clock to peripheral function in standby: Not Supported
      General: Startup speed of the HOCO in Standby and Snooze modes: Not Supported
      General: Flash mode in sleep or snooze: Not Supported
      Deep Sleep and Standby Options: Wake Sources: IRQ4
      Deep Sleep and Standby Options: Wake Sources 2: 
      Deep Sleep and Standby Options: Snooze Options (Not available on every MCU): Snooze Request Source: RXD0 falling edge
      Deep Sleep and Standby Options: Snooze Options (Not available on every MCU): Snooze End Sources: 
      Deep Sleep and Standby Options: Snooze Options (Not available on every MCU): DTC state in Snooze Mode: Disabled
      Deep Sleep and Standby Options: Snooze Options (Not available on every MCU): Snooze Cancel Source: None
      RAM Retention Control (Not available on every MCU): RAM retention in Standby mode: 
      RAM Retention Control (Not available on every MCU): TCM retention in Deep Sleep and Standby modes: Not Supported
      RAM Retention Control (Not available on every MCU): Standby RAM retention in Standby and Deep Standby modes: Not Supported
      Oscillator LDO Control (Not available on every MCU): PLL1 LDO State in standby mode: Not Supported
      Oscillator LDO Control (Not available on every MCU): PLL2 LDO State in standby mode: Not Supported
      Oscillator LDO Control (Not available on every MCU): HOCO LDO State in standby mode: Not Supported
      Deep Standby Options (Not available on every MCU): I/O Port Retention: Maintain the IO port states
      Deep Standby Options (Not available on every MCU): Power-Supply Control: Supply power to the Standby RAM, low-speed on-chip oscillator, AGTn (n = 0-3) and USBFS resume detecting unit
      Deep Standby Options (Not available on every MCU): Cancel Sources: IRQ4
      Deep Standby Options (Not available on every MCU): Cancel Edges: IRQ4 Rising Edge
      
    Instance "g_external_irq4 External IRQ (r_icu)"
      Name: g_external_irq4
      Channel: 4
      Trigger: Rising
      Digital Filtering: Disabled
      Filter Source: PCLK filter
      Digital Filtering Sample Clock (Only valid when Digital Filtering is Enabled): PCLK / 64
      Callback: user_irq4_callback
      Pin Interrupt Priority: Priority 15
      
    Instance "g_pcdc0 USB PCDC (r_usb_pcdc)"
      Name: g_pcdc0
      
      Instance "g_basic0 USB (r_usb_basic)"
        Name: g_basic0
        USB Mode: Peri mode
        USB Speed: Full Speed
        USB Module Number: USB_IP0 Port
        USB Device Class: Peripheral Communications Device Class
        USB Descriptor: g_usb_descriptor
        USB Compliance Callback: NULL
        USBFS Interrupt Priority: Priority 12
        USBFS Resume Priority: Priority 12
        USBFS D0FIFO Interrupt Priority: Priority 12
        USBFS D1FIFO Interrupt Priority: Priority 12
        USBHS Interrupt Priority: Not Supported
        USBHS D0FIFO Interrupt Priority: Not Supported
        USBHS D1FIFO Interrupt Priority: Not Supported
        USB Callback: NULL
        USB Callback Context: NULL
        
    Instance "g_flash0 Flash (r_flash_hp)"
      Name: g_flash0
      Data Flash Background Operation: Enabled
      Callback: user_flash_callback
      Flash Ready Interrupt Priority: Priority 2
      Flash Error Interrupt Priority: Priority 2
      
